Building Inspection

**Model: HT-4000**

**OVERVIEW**

The HT-4000 is a stand-alone thermo-hygrometer that has the same fast acclimating RH/T sensor found in our popular TotalCheck 3-in-1 moisture meter. For contractors who prefer having separate meters to one combination meter, the HT-4000 is the perfect solution.

**Features:**

* Bright, clear digital display.
* Relative Humidity Range: 0% - 100%,
* Temperature Range: -40°F - 255°F (-40°C - 124°C).
* Dew Point Range: -40°F - 176°F (-40°C - 80°C).
* GPP Range: 0.1 - 3820 GPP (Grains Per Pound).
* GPK Range: 0.01 - 545 GPK (Grains Per Kilogram).
* Vapor Pressure Range: 0 - 7 PSI (Pounds Per Square Inch).
* Vapor Pressure Range: 0 - 47 KPA (Kilopascals).
* Built-in back-light makes reading in dark places a cinch.
* Auto shut-off timer saves battery life.
* Reading HOLD Feature.
* Size: 8 ½” x 3 3/8” x 1 ¾”.
* Weight: 11 oz.
* Rugged construction ensures years of reliable use.
* Sturdy plastic carrying case.
* 9V battery.
* 1-year warranty.

Includes meter, (1) RH/T-S1 sensor, and carrying case. Order as HT-4000W/CS.