1. The modulating float control pilot shall be a Singer Model R400. The pilot shall be supplied with a 10” (250mm) *specify material (B62 brass or 316 stainless steel)* float rod and a 5” (127mm) diameter *specify material (polypropylene or stainless steel)* float. The pilot body shall be of Lead Free Compliant ASTM B62 bronze with Buna-N seals.