Components

2.

3.

1. ISTATION Transmitter (With power supply & antenna)

1.

1. Ethernet Cable

4.

1. DB9 Cable (Optional for POS Integration)
2. USB Keyboard (Optional)

Equipment Setup



|  |  |  |
| --- | --- | --- |
|  |  |  |
| **Step 1**Connect the antenna to the transmitter. Twist to lock in place. | **Step 2**Plug the power supply into the transmitter and then into a standard 110-240v outlet. **A surge protector is recommended for all Transmitters and Charging Bases.** | **Step 3**Plug one end of the Ethernet cable into the back of the transmitter and then the other end into your network. |

|  |  |
| --- | --- |
|  |  |
| **Step 4****OPTIONAL (For POS Integration):**Connect the serial cable to the serial port on the back of the ISTATION and then tighten the screws. | **Step 5****OPTIONAL:**Insert the USB connector from the keyboard into the back of the transmitter**.** |

**Optional items are not included unless purchased before shipping.**

System Configuration

**Please contact your IT department for assistance in setup.**

**To enter Network Programming Mode**

1. Press the “**SETUP**” button.
2. Enter the password “**6629**”followed by “**ENTER**”.
3. Once the password is accepted, the display will show “**Admin Setup”**
4. Use the following buttons to configure your transmitter.
* “**\*/MENU**” key to scroll through the different menu options.
* “**#/SELECT**” key to toggle between options.
* “**ENTER**” to edit the menu and save the new settings.
* “**CANCEL**” to exit the system programming menu.

### **Static IP Setup**

To enter the IP Address provided by your IT, follow the procedure below:

1. At the “**IP** **Address**” screen, press the “**ENTER**” key.
2. Enter the twelve-digit IP, then press the “**ENTER**” key.
3. Press the “**CANCEL**” key to exit the system programming menu or “**\*/MENU**” to scroll to the next menu.

### **DNS Setup**

To enter the DNS Server IP provided by your IT, follow the procedure below:

1. At the “**DNS Server IP**” screen, press the “**ENTER**” key.
2. Enter the twelve-digit IP, then press the “**ENTER**” key.
3. Press the “**CANCEL**” key to exit the system programming menu or “**\*/MENU**” to scroll to the next menu.

### **Client Code and Token Setup**

If you need your Client Code and Token, please contact support at 800-321-6221.

If you already have the Client Code and Token for your account, follow the procedure below:

1. At the “**SMS Text Messaging**” screen, press the “**#/SELECT**” key to turn “**ON**”.
2. Press the “**ENTER**” key.
3. At the “**SMS Company Code**” screen, use the keyboard to enter your 6-digit Client Code, then press “**ENTER**”.
4. At the “**SMS Company Token**” screen, use the keyboard to enter your 15-digit Token, then press “**Enter**”.
5. Press the “**CANCEL**” key to exit the system programming menu or “**\*/MENU**” to scroll to the next menu.

System Operation

### **Sending a direct SMS Message from your transmitter:**

To send a direct SMS Message enter the 10-digit phone number on the transmitter, then press “**ENTER**”. Use the keyboard to type the desired message, then press the “**ENTER**” key. For example, type “**8003216221-ENTER-Your table is ready. -ENTER**” to send the phone number 800-321-6221 the message Your table is ready.