**FINAL FORKLIFT TEST**

# Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_ Score: \_\_\_\_\_\_\_\_

1. Your forklift can be driven by:
2. Any employee
3. An employee who has training from another facility
4. Only operators specially trained by their company
5. When changing directions: (forward to reverse, or reverse to forward)
6. Always stop
7. Slow down to about 1 mph
8. Don't worry about speed; a forklift is built to take shock
9. Never exceed the rated load capacity of your truck:
10. Unless you add additional counterweight
11. Unless your lift is under 84 inches high
12. No, never
13. When taking a load down a ramp:
14. Drive backwards
15. Drive forwards
16. Reducing speed by zigzagging
17. If you have to park on a ramp:
18. Leave the machine in gear
19. Set the brakes and block the wheels
20. Set the load down, and rest the machine against it
21. On a forklift, your horn:
22. Makes a good device to catch the foreman's attention
23. Should be sounded at intersections
24. Should be sounded when you're stacking pallets
25. When loading a truck trailer, you should:
26. Check the trailer tires to make sure they are blocked
27. Check to make sure that the tractor is attached
28. Load the left side of the trailer first
29. When approaching a blind corner, you should:
30. Stop, and then proceed
31. Slow down, sound the horn and proceed slowly
32. Continue at same speed while sounding the horn
33. The condition of a pallet:
34. Affects load stability
35. Affects load center
36. Neither of the above
37. The speed at which a forklift should be operated is:
38. Determined by the operator
39. Determined by the load, driving conditions, and plant rules
40. Determined by signs posted along aisles and passageways
41. When operating a fully loaded sit down riding type forklift on a ramp, you should:
42. Drive up the ramp with the load in front
43. Drive up the ramp with the load trailing
44. It doesn't make a difference
45. When parking a lift truck:
46. The forks should be above eye-level to prevent an accident
47. 2" above the floor
48. Resting on the floor with the tips pointing down
49. Safety of a forklift is the responsibility of:
50. Operators
51. Management
52. Manufacturer
53. All of the above
54. After picking up a palletized load, it should be tilted:
    1. As far back as possible
    2. Only far enough back to stabilize the load
    3. Not at all
55. Forklift operator training is:
    1. Required by law
    2. Is only necessary for new operators
    3. Is valuable even if it only prevents one accident from occurring
    4. Both "a" and "c"

**True or False**

1. Your tires should be checked and seatbelt worn **every time** you use the truck.
2. A lift truck steers with its rear wheels and its rear end swings on turns.
3. It is okay to smoke when refueling as long as you are in a restricted area.
4. Start out slowly with every load.
5. Loads when lifted high reduce a truck's stability.
6. As long as you sit beside him, it is okay to let an unauthorized person operate your forklift.
7. Never let bystanders stand beneath loads when you're stacking.
8. A careful driver may hang his leg outside a machine when it is protected by a wide load.
9. A good operator drives slowly on slippery and wet floors.
10. **One** of the greatest causes of accidents is forgetting to watch overhead obstructions when lifting.
11. An overhead guard is intended to offer protection from the impact of falling **capacity** loads.
12. Never raise a fellow employee on the forks or pallets.
13. The center of the load should be situated on the tips of the load forks.
14. The operator does not have to inspect his truck after a mechanic has made repairs.
15. Forklifts should not be parked in front of stairways and fire equipment

Final Score:

Instructor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_