**VERTICAL CUTTER MIXER**

Provide one (1) **Vertical Cutter Mixer**, Model **R60T** as manufactured by **Robot Coupe USA**. Unit shall be provided with all standard features as follows:

* All stainless steel construction
* Designed for vertical cutting and mixing: mix, chop, puree, blend, mix and knead doughs
* 16 HP, two-speed (1800RPM/3600RPM) motor
* 63-qt. stainless steel bowl with integral stainless steel handles. Bowl shall tilt for easy removal of food product and shall be easily removed for cleaning.
* Polycarbonate clear lid shall be designed to allow the addition of liquids or ingredients during processing.
* Adjustable 3-blade smooth knife assembly to give equal results for small or large batches.
* Stainless steel control panel with push-type ON/OFF buttons, PULSE button and 0-15 minute digital timer.
* Open frame stainless steel design for easy cleaning.
* Magnetic safety and thermal protection, bowl detection device, lid detection device and locking lid detection devices.

Electrical requirements:

* 208-240V/60Hz/3Ph, 60 amps, NEMA 15-50 Plug

Warranty:

* One Year Parts and Labor Warranty

Additional requirements:

* Eligible bidders must visit the installation site.
* Alternates need to be submitted for approval 10 days prior to bid opening.
* Successful bidder to deliver, uncrate, set in place and remove crating.
* Local demonstration to be provided by successful bidder.