EnkaMat/ EnkaDrain Applications Chart

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Application | Enkadrain 3611R | Enkadrain 3615R | Enkadrain 3811R | Enkadrain W 3601 | Enkamat 7010 | Enkadrain 9010 | Enkavent 6128 | EnkaRetain & Drain 3111 | EnkaRetain & Drain 3211 |
| Green Roof | X | X | X | X | X |  |  |  |  |
| Green roof plant stabilization for sloped and high wind and conditions |  |  |  |  | X |  |  |  |  |
| Pre-vegetated green roof mats |  |  |  |  | X |  |  |  |  |
| Extensive green roofs |  |  |  |  |  |  |  | X | X |
| Intensive green roofs |  |  |  |  |  |  |  | X | X |
| Exterior planters | X | X | X |  |  |  |  | X | X |
| Exterior & interior planters |  |  |  |  |  |  |  | X | X |
| Foundation Walls | X | X | X | X |  |  |  |  |  |
| Plaza decks | X | X | X | X |  |  |  |  |  |
| Retaining walls | X | X | X |  |  |  |  |  |  |
| Beneath slabs | X | X | X |  |  |  |  |  |  |
| Earth sheltered homes | X | X | X |  |  |  |  |  |  |
| Underground parking | X | X | X |  |  |  |  |  |  |
| Planters |  |  |  |  |  | X |  |  |  |
| Playgrounds |  |  |  |  |  | X |  |  |  |
| Zoos |  |  |  |  |  | X |  |  |  |
| Split slab construction |  |  |  | X |  |  |  |  |  |
| Under pavers |  |  |  | X |  |  |  |  |  |
| Spacer between zinc and other metal roofs and the weather barrier underlayment/plywood substrate in sloped applications |  |  |  |  | X |  |  |  |  |
| Thermal break between metal roofs & sheathing |  |  |  |  | X |  |  |  |  |
| Spacer between ballast and loose laid, fully adhered or mechanically attached roofs |  |  |  |  | X |  |  |  |  |
| Blue roof water storage |  |  |  |  |  |  |  | X | X |
| Landfill caps |  |  |  |  |  |  |  | X | X |
| Radon mitigation under concrete slab construction |  |  |  |  |  |  |  |  |  |
| Radon mitigation in basement slab construction |  |  |  |  |  |  | X |  |  |
| Hydrostatic pressure relief |  |  |  |  |  |  | X |  |  |
|  |  |  |  |  |  |  | X |  |  |