**FOOD PROCESSOR**

Provide one (1) **Commercial Food Processor**, **Model CL51** as manufactured by **Robot Coupe USA**. Unit shall be provided with standard features as follows:

* 1.5 HP, 425 RPM, direct drive, fan-cooled motor with magnetic safety switch.
* Removable continuous feed vegetable prep lead with two deep feed openings. One for larger produce and one for smaller, more delicate produce.
* Attachments easily removed to facilitate maximum ease of cleaning.
* 3mm slicing disc and 3mm medium grating disc supplied as standard.
* Control panel equipped with push-type ON and OFF buttons.

Furnish unit with the following accessory equipment:

* 28128 Slicing Disc, 5mm
* 28130 Slicing Plate, 10mm
* 28052 Julienne Plate, 4 x 4mm
* 28112 Dicing Kit, 10 x 10mm
* 28180 Romaine Lettuce Kit
* 39881 Dice Cleaning Kit
* Four (4) additional 27258 Plate Racks

Electrical requirements:

* 120V/60/1Ph, 12 amps, NEMA 5-15

Warranty:

* 1 Year Parts and Labor Warranty

Additional requirements;

* Alternates must be submitted for approval 10 days prior to bid opening.
* Successful bidder to deliver unit to end user location.
* Local demonstration to be provided by successful bidder.