**FOOD PROCESSOR**

Provide one (1) **Commercial Food Processor**, Model **R2Dice** as manufactured by **Robot Coupe USA**. Unit shall be provided with standard features as follows:

* 2 HP, 1725 RPM, direct drive, fan-cooled motor.
* 3 Qt. “stock pot” shaped cutter bowl with handle, “S” blade, and see-through lid with introduction port to allow user to add ingredients while machine is processing.
* Continuous feed vegetable prep attachment with two deep feed openings. One for larger produce and one for smaller, more delicate produce.
* Attachments easily removed for optimum sanitization. All attachments shall be dishwasher safe.
* 4mm slicing disc, 2mm grating disc and 10mm dicing kit supplied as standard.
* Control panel equipped with push-type ON, OFF and PULSE buttons.

Furnish unit with the following accessory equipment:

* 27087 Slicing Disc, 5mm
* 27046 Grating Plate, 6mm
* 27047 Julienne Plate, 4 x 4mm
* R255 Free Standing Disc Rack
* 39881 Dice Cleaning Kit

Electrical requirements:

* 120V/60/1Ph, 13 amps, NEMA 5-15

Warranty:

* 3 Year Motor Warranty
* 1 Year Parts and Labor Warranty

Additional requirements;

* Alternates must be submitted for approval 10 days prior to bid opening.
* Successful bidder to deliver unit to end user location.
* Local demonstration to be provided by successful bidder.