**FOOD PROCESSOR**

Provide one (1) **Commercial Food Processor**, **Model R602VV** as manufactured by **Robot Coupe USA**. Unit shall be provided with standard features as follows:

* 3.0 HP, variable speed (300 – 3500 RPM), direct drive, fan-cooled motor.
* Metal motor support with metal motor base designed for heavy duty use.
* 7 Qt. stainless steel bowl with handle and stainless steel smooth “S” blade. See-through lid with introduction port to allow user to add ingredients while machine is processing.
* Removable continuous feed vegetable prep lead with two deep feed openings. One for larger produce and one for smaller, more delicate produce.
* Attachments easily removed to facilitate maximum ease of cleaning.
* Magnetic safety system and auto shut-off for maximum operator safety.
* 3mm slicing disc and 3mm medium grating disc supplied as standard.
* Control panel equipped with push-type ON and OFF buttons.

Furnish unit with the following accessory equipment:

* 28128 Slicing Disc, 5mm
* 28130 Slicing Plate, 10mm
* 28052 Julienne Plate, 4 x 4mm
* 28112 Dicing Kit, 10 x 10mm
* 28180 Romaine Lettuce Kit
* 39881 Dice Cleaning Kit
* Four (4) additional 27258 Plate Racks

Electrical requirements:

* 120V/60/1Ph, 15 amps, NEMA 5-20P

Warranty:

* 1 Year Parts and Labor Warranty

Additional requirements;

* Alternates must be submitted for approval 10 days prior to bid opening.
* Successful bidder to deliver unit to end user location.
* Local demonstration to be provided by successful bidder.